**Worksheet 10.2: Fluid Mechanics - Dynamics**

**Volume flow rate. (Av = ΔV/t) (memorize volumes of cylinders, spheres, and rectangular solids)**

1. Water flows at 0.854 m/s down a 1.59 cm diameter hose. What time will it take to fill a circular kiddie pool that is 1.75 m in diameter to a depth of 37.0 cm? (5250 s)
2. An HVAC duct that is 1.02 m in diameter supplies air to a 10.0 m x 4.20 m x 21.0 m room at a rate of 3.50 ACH. What is the air speed in the duct? (3.50 ACH means it replaces the air 3.50 times per hour, so it does it once in (3600 s)/3.5 seconds) (1.05 m/s)
3. A pump delivers 180. liters per minute. What speed does the water travel through its 4.15 cm diameter outlet pipe? What time would it take for the pump to fill a rectangular tank that is 2.1 m x 3.3 m x 5.4 m? (2.22 m/s, 12,500 s)
4. A classroom is 32.0 feet by 58.5 feet and 8.10 feet high. If air flows 8.65 f/s down a 1.50 foot x 1.00 foot air duct, what time in minutes does it take to replace the air in the room? (19.5 minutes)
5. A pipe bursts in a classroom that is 12.0 m x 35.0 m in floor area. If it is a 5.08 cm diameter pipe, and the water is going 20.3 m/s, what depth will the water be in a hour if it does not leak? (35.3 cm)

**Continuity (Av = Av)**

1. A 0.75 inch pipe with water going 4.5 inches per second narrows to 0.50 inches inner diameter. What is the velocity in the narrow part? (10. inches/sec)
2. Air flows at 0.450 m/s down a duct that is 24.0 cm x 62.0 cm. If it widens to 35.0 x 62.0 cm, what is the air velocity there? (0.309 m/s)
3. A circular 2.50 cm diameter pipe has a flow velocity of 56.0 cm/s. What is the diameter of the pipe if the flow velocity slows to 13.0 cm/s? (5.19 cm)
4. A fire hose sprays water at 34.0 m/s out of a nozzle that is 2.50 cm in diameter. What is the diameter of the supply line if the velocity is 3.68 m/s (7.60 cm)
5. A river with a strangely rectangular channel is 20.0 m wide. At a spot where it is 6.30 m deep, the water moves at a stately 0.0850 m/s. Later there is a rapids where the water moves at 3.20 m/s. How deep is it there on the average? (Assume the channel is more or less rectangular in cross section) (0.167 m)

**Bernoulli - 2 or 3 terms: (P + ρgh + ½ρv2 = P + ρgh + ½ρv2)**

**1.00 atm = 1.013x105 Pa = 101.3 kPa = 760. Torr = 14.7 psi, ρwater = 1000. kgm-3, ρair = 1.29 kgm-3**

1. Water issues from hole in the side of a water tank at 12.0 m/s. What is the height of the water in the tank above the hole? (ρ = 1000. kgm-3) Assume atmospheric pressure above the water in the tank and at the hole. (7.34 m)
2. Air (ρ = 1.29 kgm-3) streams at 6.70 m/s through a hole in a wall. What is the pressure difference from one side to the other? (29.0 Pa)
3. The air is traveling at 45.0 m/s over the top of a wing, and 43.0 m/s over the bottom of a wing. What is the pressure difference from one side to the other? (114 Pa)
4. Water is at 1.035x105 Pa in a level pipe where the velocity is 2.40 m/s. If the pressure drops to 1.024x105 Pa, what is the velocity? (2.82 m/s)
5. Water moves at 1.70 m/s down a level pipe at a pressure of 1.015x105 Pa. What is the pressure if the water speeds up to 4.92 m/s? (9.08x104 Pa)

**Bernoulli - complex**

1. Water flows at 4.50 m/s down a 2.10 cm diameter pipe at a pressure of 9.92x104 Pa in the crawlspace. When the pipe is 1.20 m higher than this the pressure is 9.52x104 Pa. What is the velocity of the water in the pipe? What is the pipe diameter? (2.17 m/s, 3.02 cm)
2. Water moves at 3.50 m/s down a 4.80 cm diameter pipe at an elevation of 3.80 m and a pressure of 1.26x105 Pa. At a different elevation the pipe narrows to 3.60 cm in diameter and is at a pressure of 1.36x105 Pa. What is the elevation here? (1.43 m)
3. A 5.40 cm diameter pipe carries water at 3.70 m/s at an elevation of 3.40 m and a pressure of 1.56x105 Pa. At an elevation of 4.60 m the pipe narrows to 4.20 cm in diameter. What is the pressure in this part of the pipe? (1.32x105 Pa)
4. A 3.50 cm diameter pipe carries water at 4.10 m/s at an elevation of 6.30 m and a pressure of 1.24x105 Pa. The pipe widens out at an elevation of 5.10 m where the pressure is 1.43x105 Pa. What is the velocity here and the diameter of the pipe? (1.53 m/s and 5.72 cm)
5. Water moves at 4.90 m/s down a 4.70 cm diameter pipe at an elevation of 3.80 m and a pressure of 1.21x105 Pa. At a different elevation the pipe widens to 5.90 cm in diameter and is at a pressure of 1.37x105 Pa. What is the elevation here? (2.90 m)

**Stokes law: FD = 6πηrv, at terminal velocity = mg = ρVg.**

**(Ignore the buoyant force of air, but not the buoyant force of water.)**

**1 micron = 1x10-6 m = 1 µm**

**Water: ρ = 1000. kgm-3, η = 1.002x10-3 Pa s. Air: ρ = 1.29 kgm-3, η = 1.81x10-5 Pa s at 20 oC**

1. A droplet of water is 6.12 µm in diameter. What is its mass? What is its weight? What speed must it fall through air so that its Stokes drag is equal to its weight? (This is its terminal velocity) (1.20x10-13 kg, 1.18x10-12 N, 0.00113 m/s)
2. A droplet of mist falls through air with a terminal velocity of 0.00156 m/s. What is its radius? (Ignore the buoyant force of the air) (3.60 μm)
3. A tiny grain of basalt (ρ = 2920 kgm-3) is 2.20 microns in diameter. What speed does it settle in water? (Don't ignore the buoyant force of water) (5.05x10-6 m/s)
4. A tiny grain of basalt (ρ = 2920 kgm-3) takes 27.0 minutes to settle from the top of a 8.50 cm tall test tube full of water to the bottom. What is its speed? What is its radius? What time would it take to settle in a 5.40 cm radius centrifuge spinning at 1200 RPM? (5.25x10-5 m/s, 3.54x10-6 m, 18.6 s)
5. A 3.60 micron diameter particle falls through air with a terminal velocity of 0.00130 m/s. What is its density? (3330 kgm-3)

**Reynolds number Re\_r = vrρ/η**

1. Syrup with a viscosity of 1.20 Pa s and a density of 1080 kgm-3 needs to have turbulent flow down a pipe where it is heated. What speed must it go down a pipe that is 68.0 cm in diameter to ensure that it has a Re\_r of 1200? (3.92 m/s)
2. What is the Re\_r of water flowing at 0.130 m/s down a tube that is 8.01 mm in diameter? (520.)
3. What is the maximum speed air can flow down a 24.0 cm diameter duct to have a Re\_r of 850? (9.94 cm/s)
4. What is the Re\_r of air flowing at 0.935 m/s down a duct with a diameter of 1.20 m? (4.00x104)
5. What maximum diameter pipe can water flow down at 0.890 m/s to have a Re\_r of 950? (2.14 mm)